**## Factors Affecting Charging Station Location**

The decision regarding the ideal placement of Electric Vehicle Charging Stations (EVCS) is a sophisticated process encompassing a plethora of considerations. There are several interrelated quantitative and qualitative factors influencing this decision, including but not limited to operator economics, driver satisfaction, vehicle power loss, traffic congestion, and power grid safety [1].

Falvo et al.'s work illustrates the role of reducing energy consumption by exploiting the capabilities of existing power plants. They draw attention to the interconnectivity of different transportation systems - EVs and subways - highlighting the potential for symbiotic relationships to optimize power usage. Their research sheds light on the strategic importance of aligning EVCS locations with the current power grid, not just for energy efficiency, but also for operational economics and grid safety. It serves as a reminder that the placement of charging stations should be an integral part of broader urban energy planning [2].

Guo et al. present an alternative approach to the problem, employing a fuzzy TOPSIS method for the assessment of potential locations. Their approach takes into account not just practical or economic factors, but a broad array of environmental, economic, and social benchmarks. This underscores the importance of a holistic, multifaceted evaluation process for locating EVCS. Beyond the fundamental requirements of power supply and accessibility, Guo et al. emphasize the need to assess the broader societal impact, environmental implications, and economic viability of potential locations. These findings underscore the fact that the decision-making process should not be limited to infrastructure and logistics alone but should strive to align with wider sustainable development goals [3].

Similarly, Asamer et al. propose a comprehensive, integrative approach to the placement of EVCS. They contend that several variables - ranging from environmental conditions to the availability of power and legislative considerations - must be factored into the decision-making process. Significantly, they also highlight the importance of empirical data, employing taxi data as a proxy to assess charging demand. The utilization of real-world data, they suggest, can provide invaluable insights into patterns of use and potential demand hotspots, thus allowing for more targeted and effective placement of charging stations [4].

Building upon this foundation, Zhu et al. introduce an economic perspective into the analysis, evaluating how costs - both to the user and those associated with the establishment and operation of the charging stations - impact the final number and location of EVCS. This underscores the need for a detailed cost-benefit analysis as part of the decision-making process. It also raises an important question of user satisfaction and accessibility, emphasizing that the locations need to be convenient for the end users to encourage uptake and continued use of EVs [5].

Complementing these perspectives, Sun et al. propose an innovative, user-centric approach. They consider residents' travel patterns, categorizing them as either short-distance or long-distance travelers. This differentiation aids in determining not only the optimal location for charging stations but also the appropriate number of stations needed. It serves as a reminder that the deployment of EVCS should not be a one-size-fits-all solution. Instead, it should be tailored to meet the specific needs and habits of local residents, thereby ensuring maximum usability and efficacy [6].

In summary, the complex interplay of factors affecting the location of EVCS necessitates a multifaceted and integrative approach. The aforementioned studies underline the need for strategies that balance technical requirements, economic feasibility, societal impact, and end-user needs. It is through this careful balancing act that the optimal location for EVCS can be determined, thereby promoting widespread EV adoption and the resultant environmental benefits. The findings from these studies collectively demonstrate that the placement of EVCS is an intricate process, interweaving numerous factors and requiring comprehensive, multidimensional planning and assessment [1] - [6].#

**### Optimization Models for EV Charging Station Distribution**

This section discusses various optimization models proposed by researchers for the distribution of Electric Vehicle Charging Stations (EVCS). These models consider a broad spectrum of factors to help enhance the adoption of Electric Vehicles (EVs) and user satisfaction.

Frade et al. used a maximal covering model to identify potential demand areas and possible EVCS locations in Lisbon, aiming to maximize covered demands [7]. He et al. proposed a double-layer mathematical model considering vehicle driving distances and charging demands, underlining the importance of daily mobility patterns of EV users [8].

Shahraki et al. presented an optimization model maximizing vehicle mileage based on driving patterns, emphasizing the role of real-world data in location decisions [9]. Wu et al. designed a stochastic flow capturing location model reflecting the randomness in EV users' traveling behavior [10].

Models by Tu et al. and Luo et al. included temporal and spatial constraints, making these models more realistic by considering variable parking availability, congestion levels, and EV owners' home and work locations [11] [12].

Battery characteristics have been factored into models by Liu et al. and Mehrjerdi et al., highlighting the need for different strategies for different charging applications, and the importance of power and capacity of charging facilities [13] [14].

He et al. and Davidov et al. incorporated economic aspects in their models, considering costs such as battery, charging station, and energy storage system expenses [15] [16].

Hosseini and Sarder, and Chen et al. integrated both quantitative and qualitative aspects into their models, underlining the importance of subjective factors and user experience [17] [18].

Zeng et al. integrated human behavior into their station-level optimization framework, pointing out that station networks must accommodate user preferences [19].

Hodgson and Kuby and Lim further refined the models by considering EV charging during long trips and the limited range of EVs, which resulted in the Flow Refueling Location Problem (FRLP) [20] [21] [7].

The FRLP model has been extended to consider limited charging station capacity, alternative paths, different types of stations and vehicles, and congestion at stations [22] [23] [24] [25] [26] [27] [28]. Multi-period deterministic extensions of FRLP have been suggested, allowing for dynamic opening of new stations and considering limited station capacity [29] [30].

Few studies have addressed uncertainties in EV charging infrastructure planning, such as unpredictable driving range or variability in recharging demand. Some recent works have introduced the concept of portable charging stations and advocated for robust optimization approaches [31] [32] [33] [34] [35] .

These diverse models demonstrate the multi-faceted nature of EVCS placement and the need for comprehensive, flexible approaches incorporating demand characteristics, technical specifications, cost factors, and human behaviors to promote EV adoption and environmental benefits [7] - [19].

**## Algorithm for Optimal EV Charging Station Configuration**

article discusses various optimization techniques used to determine optimal configurations of Electric Vehicle Charging Stations (EVCS). The methods include optimization methods, genetic algorithms, decomposition algorithms, clustering methods, and combinations of these techniques.

Sadeghi-Barzani et al. used a mixed-integer non-linear programming (MINLP) optimization method and a genetic algorithm to find optimal EVCS location and scale [36]. Arslan et al. utilized the Benders decomposition algorithm to optimize EVCS location, aiming to maximize mileage and minimize transportation costs [37].

Zhang et al. introduced a decentralized valley-filling charging strategy that used a cost minimization pricing scheme, emphasizing the importance of pricing mechanisms [38]. Dong et al. applied the SNN clustering algorithm for optimizing EVCS placement on expressways [YYY].

Zhu et al. and Akbari et al. used genetic algorithms for optimizing EVCS locations, acknowledging the interplay between technical specifications, user charging demand, and spatial factors [39] [40]. Awasthi et al. combined a genetic algorithm with particle swarm optimization for determining optimal EVCS location and size [41].

Particle swarm optimization algorithms have been used by Li et al. and Chen et al. to determine EVCS deployment strategy and charging facility distribution [XXXX] [42]. Clustering methods like k-means cluster analysis were employed by Zhang et al. and Straka et al. to understand dynamic charging demand trends and user behavior [43] [44].

Wu et al. used approximate dynamic programming and an evolutionary algorithm to determine optimal charging start times for EVs, demonstrating the interest in smart charging strategies [45].

Despite these advancements, the article identifies gaps, including the lack of comprehensive analyses considering total social cost, underutilization of genetic algorithms, and limited case studies of specific charging station scenarios, like those in Ireland.

To address these gaps, the article proposes an optimal distribution model of EVCS based on total social cost, utilizing a genetic algorithm for iterative simulation. This model deviates from traditional reliance on Euclidean distance and includes a road bending coefficient. The article also incorporates a case study of Ireland, reflecting actual EV charging demand in five major cities. This approach provides a promising direction for future EVCS optimization research [36] - [45].

# Bibliography

|  |  |
| --- | --- |
| [1] | W. Kong, Y. Luo, G. Feng, K. Li and H. Peng, "Optimal location planning method of fast charging station for electric vehicles considering operators, drivers, vehicles, traffic flow and power grid," *Energy,* vol. 186, 2019. |
| [2] | M. C. Falvo, R. Lamedica, R. Bartoni and G. Maranzano, "Energy management in metro-transit systems: An innovative proposal toward an integrated and sustainable urban mobility system including plug-in electric vehicles," *Electric Power Systems Research,* vol. 81, no. 12, pp. 2127-2138, 2011. |
| [3] | S. Guo and H. Zhao, "Optimal site selection of electric vehicle charging station by using fuzzy TOPSIS based on sustainability perspective," *Applied Energy,* vol. 158, pp. 390-402, 2015. |
| [4] | J. Asamer, M. Reinthaler, M. Ruthmair, M. Straub and J. Puchinger, "Optimizing charging station locations for urban taxi providers," *Transportation Research Part A: Policy and Practice,* vol. 85, pp. 233-246, 2016. |
| [5] | Z. Zhu, Z. Gao, J. Zheng and H. Du, "Charging Station Planning for Plug-In Electric Vehicles," *Journal of Systems Science and Systems Engineering,* vol. 27, pp. 24-45, 2018. |
| [6] | Z. Sun, W. Gao, B. Li and L. Wang, "Locating charging stations for electric vehicles," *Transport Policy,* vol. 98, pp. 48-54, 2020. |
| [7] | I. Frade, A. Ribeiro and A. Antunes, "Optimal Location of Charging Stations for Electric Vehicles in a Neighborhood in Lisbon, Portugal," *Transportation Research Record: Journal of the Transportation Research Board,* vol. 2252, no. 1, 2011. |
| [8] | F. He, Y. Yin and J. Zhou, "Deploying public charging stations for electric vehicles on urban road networks," *Transportation Research Part C: Emerging Technologies,* vol. 60, pp. 227-240, 2015. |
| [9] | N. Shahraki, H. Cai, M. Turkay and M. Xu, "Optimal locations of electric public charging stations using real world vehicle travel patterns," *Transportation Research Part D: Transport and Environment,* vol. 41, pp. 165-176, 2015. |
| [10] | F. Wu and R. Sioshansi, "A stochastic flow-capturing model to optimize the location of fast-charging stations with uncertain electric vehicle flows," *Transportation Research Part D: Transport and Environment,* vol. 53, pp. 354-376, 2017. |
| [11] | W. Tu, Q. Li, Z. Fang, S. Shaw, B. Zhou and X. Chang, "Optimizing the locations of electric taxi charging stations: A spatial–temporal demand coverage approach," *Transportation Research Part C: Emerging Technologies,* vol. 65, pp. 172-189, 2016. |
| [12] | L. Luo, W. Gu, S. Zhou, H. Huang, S. Gao, J. Han, Z. Wu and X. Dou, "Optimal planning of electric vehicle charging stations comprising multi-types of charging facilities," *Applied Energy,* vol. 226, pp. 1087-1099, 2018. |
| [13] | K. Liu, L. Kang, H. Ma, J. Zhang and Q. Peng, "Multi-objective optimization of charging patterns for lithium-ion battery management," *Energy Conversion and Management,* vol. 159, pp. 151-162, 2018. |
| [14] | H. Mehrjerdi and R. Hemmati, "Electric vehicle charging station with multilevel charging infrastructure and hybrid solar-battery-diesel generation incorporating comfort of drivers," *Journal of Energy Storage,* vol. 26, 2019. |
| [15] | Y. He, Z. Song and Z. Liu, "Fast-charging station deployment for battery electric bus systems considering electricity demand charges," *Sustainable Cities and Society,* vol. 48, 2019. |
| [16] | S. Davidov and M. Pantos, "Optimization model for charging infrastructure planning with electric power system reliability check," *Energy,* vol. 166, pp. 886-894, 2019. |
| [17] | S. Hosseini and M. Sarder, "Development of a Bayesian network model for optimal site selection of electric vehicle charging station," *International Journal of Electrical Power & Energy Systems,* vol. 105, pp. 110-122, 2019. |
| [18] | R. Chen, X. Qian, L. Miao and S. V. Ukkusuri, "Optimal charging facility location and capacity for electric vehicles considering route choice and charging time equilibrium," *Computer & Operations Research,* vol. 113, 2020. |
| [19] | T. Zeng, S. Bae, B. Travacca and S. Moura, "Inducing Human Behavior to Maximize Operation Performance at PEV Charging Station," *IEEE Transactions on Smart Grid,* vol. 12, no. 4, pp. 3353-3363, 2021. |
| [20] | M. J. Hodgson, "A Flow Capturing Location Allocation Model," *Geographical Analysis,* vol. 22, no. 3, pp. 270-279, 1990. |
| [21] | M. Kuby and S. Lim, "The flow-refueling location problem for alternative-fuel vehicles," *Socio-Economic Planning Sciences,* vol. 39, no. 2, pp. 125-145, 2005. |
| [22] | C. Upchurch and M. Kuby, "A Model for Location of Capacitated Alternative-Fuel Stations," *Geographical Analysis,* vol. 41, no. 1, pp. 85-106, 2009. |
| [23] | M. Hosseini and S. A. MirHassan, "A heuristic algorithm for optimal location of flow-refueling capacitated stations," *International Transactions in Operational Research,* vol. 24, pp. 1377-1403, 2017. |
| [24] | B. Yildiz, B. Arslan and O. E. Karaan, "A branch and price approach for routing and refueling station location model," *European Journal of Operational Research,* vol. 248, no. 3, pp. 815-826, 2016. |
| [25] | S. Li, Y. Huang and S. J. Mason, "A multi-period optimization model for the deployment of public electric vehicle charging stations on network," *Transportation Research Part C,* vol. 65, pp. 128-143, 2016. |
| [26] | Y. W. Wang and C. C. Lin, "Locating multiple types of recharging stations for battery-powered electric vehicle transport," *Transportation Research Part E,* vol. 58, pp. 76-87, 2013. |
| [27] | O. Arslan and O. E. Karasan, "A Benders decomposition approach for the charging station location problem with plug-in hybrid electric vehicles," *Transportation Research Part B,* vol. 93, pp. 670-695, 2016. |
| [28] | M. Ghamami, A. Zockaie and Y. M. Nie, "general corridor model for designing plug-in electric vehicle charging infrastructure," *Transportation Research Part C,* vol. 68, pp. 389-402, 2016. |
| [29] | S. H. Chung and C. Kwon, "Multi-period planning for electric car charging station locations: a case of Korean expressways," *European Journal of Operational Research,* vol. 242, no. 2, pp. 677-687, 2015. |
| [30] | A. Zhang, J. Kang and C. Kwon, "Incorporating demand dynamics in multi-period capacitated fast-charging location planning for electric vehicles," *Transportation Research Part B,* vol. 103, pp. 5-29, 2017. |
| [31] | H. De Vries and H. Duijzer, "Incorporating driving range variability in network design for refueling facilities," *Omega,* vol. 69, pp. 102-114, 2017. |
| [32] | C. Lee and J. Han, "Benders-and-price approach for electric vehicle charging station location problem under probabilistic travel range," *Transportation Research Part B,* vol. 106, pp. 130-152, 2017. |
| [33] | M. Hosseini and S. A. MirHassani, "Refueling-station location problem under uncertainty," *Transportation Research Part E,* vol. 84, pp. 101-116, 2015. |
| [34] | F. Wu and R. Sioshansi, "A stochastic flow-capturing model to optimize the location of fast-charging stations with uncertain," *Transportation Research Part D,* vol. 53, pp. 354-376, 2017. |
| [35] | M. Miralinaghi, Y. Lou, B. B. Keskin and A. Zarrinmehr, "Refueling station location problem with traffic deviation considering route choice and demand uncertainty," *International Journal of Hydrogen Energy,* vol. 42, no. 5, pp. 3335-3351, 2017. |
| [36] | P. Sadeghi-Barzani, A. Rajabi-Ghahnavieh and H. Kazemi-Karegar, "Optimal fast charging station placing and sizing," *Applied Energy,* vol. 125, pp. 289-299, 2014. |
| [37] | O. Arslan and O. Karasan, "A Benders decomposition approach for the charging station location problem with plug-in hybrid electric vehicles," *Transportation Research Part B: Methodological,* vol. 93, no. A, pp. 670-695, 2016. |
| [38] | K. Zhang, L. Xu, M. Ouyang, H. Wang, L. Lu, J. Li and Z. Li, "Optimal decentralized valley-filling charging strategy for electric vehicles," *Energy Conversion and Management,* vol. 78, pp. 537-550, 2014. |
| [39] | Z. Zhu, Z. Gao, J. Zheng and H. Du, "Charging station location problem of plug-in electric vehicles," *Journal of Transport Geography,* vol. 52, pp. 11-22, 2016. |
| [40] | M. Akbari, M. Brenna and M. Longo, "Optimal Locating of Electric Vehicle Charging Stations by Application of Genetic Algorithm," *Sustainability,* vol. 10, no. 4, 2018. |
| [41] | A. Awasthi, K. Venkitusamy, S. Padmanaban, R. Selvamuthukumaran, F. Blaabjerg and A. K. Singh, "Optimal planning of electric vehicle charging station at the distribution system using hybrid optimization algorithm," *Energy,* vol. 113, pp. 70-78, 2017. |
| [42] | Y. Chen, C. Cheng, S. Li and C. Yu, "Location optimization for multiple types of charging stations for electric scooters," *Applied Soft Computing,* vol. 67, pp. 519-528, Applied Soft Computing. |
| [43] | Y. Zhang, Q. Zhang, A. Farnoosh, S. Chen and Y. Li, "GIS-Based Multi-Objective Particle Swarm Optimization of charging stations for electric vehicles," *Energy,* vol. 169, pp. 844-853, 2019. |
| [44] | M. Straka and L. Buzna, "Clustering algorithms applied to usage related segments of electric vehicle charging stations," *Transportation Research Procedia,* vol. 40, pp. 1576-1582, 2019. |
| [45] | Y. Wu, A. Ravey, D. Chrenko and A. Miraoui, "Demand side energy management of EV charging stations by approximate dynamic programming," *Energy Conversion and Management,* vol. 196, pp. 878-890, 2019. |
| [46] | J. Zhou, Y. Wu, C. Wu, F. He, B. Zhang and F. Liu, "A geographical information system based multi-criteria decision-making approach for location analysis and evaluation of urban photovoltaic charging station: A case study in Beijing," *Energy Conversion and Management,* vol. 205, 2020. |