

**Analysis and Optimization of the**

**Charging Station Network in Germany**

Scientific work for the attainment of the degree

Master of Science

at the TUM School of Management

of the Technical University of Munich

Examiner: Univ.-Prof. Dr. Dr. h. c. mult. Horst Wildemann

Research Institute

Corporate management, logistics and production

Supervisor: Sebastian Junker M.Sc.

Course of study: Master TUM-BWL

Submitted by: Giovanni Filomeno

Arcistraße 21

80333 Munich

Matricula 03669006

Submitted on:

Table of contents

[Table of contents I](#_Toc140833074)

[List of figures II](#_Toc140833075)

[List of tables III](#_Toc140833076)

[1. Introduction 4](#_Toc140833077)

[1.1 Anxiety of Range 4](#_Toc140833078)

[1.2 The infrastructure-EV Adoption Nexus 4](#_Toc140833079)

[1.3 The Role of Government Policies and Regulations 4](#_Toc140833080)

[1.4 EV Prices, Battery Capacity and Charging Infrastructure 4](#_Toc140833081)

[1.5 Factors Affecting Charging Station Location 5](#_Toc140833082)

[1.6 Optimization Models for EV Charging Station Distribution 6](#_Toc140833083)

[1.7 Algorithm for Optimal EV Charging Station Configuration 8](#_Toc140833084)

[2. Model and Analysis 10](#_Toc140833085)

[2.1 Network Theory 10](#_Toc140833086)

[2.1.1 Diameter 10](#_Toc140833087)

[2.1.2 Average Distance 10](#_Toc140833088)

[2.1.3 Average Clustering 11](#_Toc140833089)

[2.2 Genetic Algorithm 12](#_Toc140833090)

[2.2.1 Process 12](#_Toc140833091)

[2.2.2 Variants 14](#_Toc140833092)

[2.2.3 Strengths and Weakness of Genetic Algorithms 15](#_Toc140833093)

[2.3 Interpolations Methods 15](#_Toc140833094)

[2.4 Model Overview 15](#_Toc140833095)

[2.4.1 Initial Population 15](#_Toc140833096)

[3. Results 17](#_Toc140833097)

[3.1 Pre-Processing 17](#_Toc140833098)

[3.2 Data analysis 18](#_Toc140833099)

[3.3 Network construction 19](#_Toc140833100)

[3.4 Optimization 24](#_Toc140833101)

[4. Conclusion and Further Implementations 24](#_Toc140833102)

[Bibliography IV](#_Toc140833103)

List of figures

[Figure 1: Initial population on Wave function 13](#_Toc140833104)

[Figure 2: Selected individuals from the initial population (cf. Figure 1). The individuals closest to the peak are preserved since they have the best fitness 14](#_Toc140833105)

[Figure 3: Cumulative histogram per year 18](#_Toc140833106)

[Figure 4: Cumulative histogram per year divided into Normal and Fast charging 19](#_Toc140833107)

[Figure 5: Power clustering histogram per year 19](#_Toc140833108)

[Figure 6: Charging Type clustering per year 19](#_Toc140833109)

[Figure 7: Evolution of the charging station network in Germany from 2009 to 2022 23](#_Toc140833110)

# List of tables

[Table 1: Characteristics of the different network created 21](#_Toc140833111)

# Introduction

The transformation of the global automobile industry toward electric mobility is underway. A critical factor influencing this trend is the availability and accessibility of Electric Vehicle (EV) charging infrastructure. It has been widely studied and proven that the prevalence of charging stations strongly influences the acceptance and adoption of EVs [1] [2] [3] [4].

## Anxiety of Range

The phenomenon termed as "range anxiety" is a common concern among potential EV owners. Range anxiety refers to the worry that an EV has insufficient reach to get to its destination and would leave the driver stranded. It is one of the key barriers to EV adoption [5]. This fear can be mitigated by the availability of a comprehensive, convenient, and reliable charging network, thus directly linking EV market penetration to charging infrastructure [6].

## The infrastructure-EV Adoption Nexus

Studies have demonstrated a strong correlation between the availability of public charging stations and the adoption of EVs. [4] conducted a study in the U.S, showing that the existence of public charging infrastructure positively correlates with EV uptake. When charging infrastructure was more available and accessible, the likelihood of consumers purchasing an EV increased. Moreover, [7] examined the influence of various factors on international electric vehicle policies and EV sales in 30 countries. They found that charging infrastructure was one of the most substantial determinants of national electric vehicle market share [8].

## The Role of Government Policies and Regulations

Government policies also play a crucial role in the proliferation of charging stations and consequently, the promotion of EV adoption. Incentives like grants, subsidies, and tax reductions have been applied in various countries to accelerate the deployment of EV charging stations [9]. Such policy measures have had a substantial impact on both the expansion of charging infrastructure and the adoption of electric vehicles.

## EV Prices, Battery Capacity and Charging Infrastructure

While the charging infrastructure is a significant factor, other elements like EV prices, government subsidies, and battery capabilities are also key contributors to EV market penetration [9]. Reduction in battery prices and improvements in battery technology have increased the affordability and driving range of EVs, thereby supporting the growth of the EV market. Nevertheless, without an extensive and reliable charging network, widespread EV adoption remains a challenge.

## Factors Affecting Charging Station Location

The decision regarding the ideal placement of Electric Vehicle Charging Stations (EVCS) is a sophisticated process encompassing a plethora of considerations. There are several interrelated quantitative and qualitative factors influencing this decision, including but not limited to operator economics, driver satisfaction, vehicle power loss, traffic congestion, and power grid safety [10].

Falvo et al.'s work illustrates the role of reducing energy consumption by exploiting the capabilities of existing power plants. They draw attention to the interconnectivity of different transportation systems - EVs and subways - highlighting the potential for symbiotic relationships to optimize power usage. Their research sheds light on the strategic importance of aligning EVCS locations with the current power grid, not just for energy efficiency, but also for operational economics and grid safety. It serves as a reminder that the placement of charging stations should be an integral part of broader urban energy planning [11].

Guo et al. present an alternative approach to the problem, employing a fuzzy TOPSIS method for the assessment of potential locations. Their approach takes into account not just practical or economic factors, but a broad array of environmental, economic, and social benchmarks. This underscores the importance of a holistic, multifaceted evaluation process for locating EVCS. Beyond the fundamental requirements of power supply and accessibility, Guo et al. emphasize the need to assess the broader societal impact, environmental implications, and economic viability of potential locations. These findings underscore the fact that the decision-making process should not be limited to infrastructure and logistics alone but should strive to align with wider sustainable development goals [12].

Similarly, Asamer et al. propose a comprehensive, integrative approach to the placement of EVCS. They contend that several variables - ranging from environmental conditions to the availability of power and legislative considerations - must be factored into the decision-making process. Significantly, they also highlight the importance of empirical data, employing taxi data as a proxy to assess charging demand. The utilization of real-world data, they suggest, can provide invaluable insights into patterns of use and potential demand hotspots, thus allowing for more targeted and effective placement of charging stations [13].

Building upon this foundation, Zhu et al. introduce an economic perspective into the analysis, evaluating how costs - both to the user and those associated with the establishment and operation of the charging stations - impact the final number and location of EVCS. This underscores the need for a detailed cost-benefit analysis as part of the decision-making process. It also raises an important question of user satisfaction and accessibility, emphasizing that the locations need to be convenient for the end users to encourage uptake and continued use of EVs [14].

Complementing these perspectives, Sun et al. propose an innovative, user-centric approach. They consider residents' travel patterns, categorizing them as either short-distance or long-distance travelers. This differentiation aids in determining not only the optimal location for charging stations but also the appropriate number of stations needed. It serves as a reminder that the deployment of EVCS should not be a one-size-fits-all solution. Instead, it should be tailored to meet the specific needs and habits of local residents, thereby ensuring maximum usability and efficacy [15].

In summary, the complex interplay of factors affecting the location of EVCS necessitates a multifaceted and integrative approach. The aforementioned studies underline the need for strategies that balance technical requirements, economic feasibility, societal impact, and end-user needs. It is through this careful balancing act that the optimal location for EVCS can be determined, thereby promoting widespread EV adoption and the resultant environmental benefits. The findings from these studies collectively demonstrate that the placement of EVCS is an intricate process, interweaving numerous factors and requiring comprehensive, multidimensional planning and assessment [10] - [15].

## Optimization Models for EV Charging Station Distribution

This section discusses various optimization models proposed by researchers for the distribution of Electric Vehicle Charging Stations (EVCS). These models consider a broad spectrum of factors to help enhance the adoption of Electric Vehicles (EVs) and user satisfaction.

Frade et al. used a maximal covering model to identify potential demand areas and possible EVCS locations in Lisbon, aiming to maximize covered demands [16]. He et al. proposed a double-layer mathematical model considering vehicle driving distances and charging demands, underlining the importance of daily mobility patterns of EV users [17].

Shahraki et al. presented an optimization model maximizing vehicle mileage based on driving patterns, emphasizing the role of real-world data in location decisions [18]. Wu et al. designed a stochastic flow capturing location model reflecting the randomness in EV users' traveling behavior [19].

Models by Tu et al. and Luo et al. included temporal and spatial constraints, making these models more realistic by considering variable parking availability, congestion levels, and EV owners' home and work locations [20] [21].

Battery characteristics have been factored into models by Liu et al. and Mehrjerdi et al., highlighting the need for different strategies for different charging applications, and the importance of power and capacity of charging facilities [22] [23].

He et al. and Davidov et al. incorporated economic aspects in their models, considering costs such as battery, charging station, and energy storage system expenses [24] [25].

Hosseini and Sarder, and Chen et al. integrated both quantitative and qualitative aspects into their models, underlining the importance of subjective factors and user experience [26] [27].

Zeng et al. integrated human behavior into their station-level optimization framework, pointing out that station networks must accommodate user preferences [28].

Hodgson and Kuby and Lim further refined the models by considering EV charging during long trips and the limited range of EVs, which resulted in the Flow Refueling Location Problem (FRLP) [29] [30] [16].

The FRLP model has been extended to consider limited charging station capacity, alternative paths, different types of stations and vehicles, and congestion at stations [31] [32] [33] [34] [35] [36] [37]. Multi-period deterministic extensions of FRLP have been suggested, allowing for dynamic opening of new stations and considering limited station capacity [38] [39].

Few studies have addressed uncertainties in EV charging infrastructure planning, such as unpredictable driving range or variability in recharging demand. Some recent works have introduced the concept of portable charging stations and advocated for robust optimization approaches [40] [41] [42] [43] [44] .

These diverse models demonstrate the multi-faceted nature of EVCS placement and the need for comprehensive, flexible approaches incorporating demand characteristics, technical specifications, cost factors, and human behaviors to promote EV adoption and environmental benefits [16] - [28].

## Algorithm for Optimal EV Charging Station Configuration

This section discusses various optimization techniques used to determine optimal configurations of Electric Vehicle Charging Stations (EVCS). The methods include optimization methods, genetic algorithms, decomposition algorithms, clustering methods, and combinations of these techniques.

Sadeghi-Barzani et al. used a mixed-integer non-linear programming (MINLP) optimization method and a genetic algorithm to find optimal EVCS location and scale [45]. Arslan et al. utilized the Benders decomposition algorithm to optimize EVCS location, aiming to maximize mileage and minimize transportation costs [46].

Zhang et al. introduced a decentralized valley-filling charging strategy that used a cost minimization pricing scheme, emphasizing the importance of pricing mechanisms [47]. Dong et al. applied the SNN clustering algorithm for optimizing EVCS placement on expressways [YYY].

Zhu et al. and Akbari et al. used genetic algorithms for optimizing EVCS locations, acknowledging the interplay between technical specifications, user charging demand, and spatial factors [48] [49]. Awasthi et al. combined a genetic algorithm with particle swarm optimization for determining optimal EVCS location and size [50].

Particle swarm optimization algorithms have been used by Li et al. and Chen et al. to determine EVCS deployment strategy and charging facility distribution [XXXX] [51]. Clustering methods like k-means cluster analysis were employed by Zhang et al. and Straka et al. to understand dynamic charging demand trends and user behavior [52] [53].

Wu et al. used approximate dynamic programming and an evolutionary algorithm to determine optimal charging start times for EVs, demonstrating the interest in smart charging strategies [54].

Despite these advancements, the article identifies gaps, including the lack of comprehensive analyses considering total social cost, underutilization of genetic algorithms, and limited case studies of specific charging station scenarios, like those in Ireland.

To address these gaps, the article proposes an optimal distribution model of EVCS based on total social cost, utilizing a genetic algorithm for iterative simulation. This model deviates from traditional reliance on Euclidean distance and includes a road bending coefficient. The article also incorporates a case study of Ireland, reflecting actual EV charging demand in five major cities. This approach provides a promising direction for future EVCS optimization research [45] - [54].

# Model and Analysis

## Network Theory

### Diameter

The diameter of a graph is a fundamental concept in the field of graph theory, offering significant insights into the overall structural properties of the graph. In a formal sense, the diameter of a graph is defined as the greatest shortest path length between any pair of vertices within the graph. It signifies the longest of all the shortest paths which can be navigated from one vertex to any other vertex within the graph [55]. To express this mathematically, let's denote a graph as , where is the set of vertices and is the set of edges present in the graph. For any pair of vertices, and in , let denote the shortest path distance between these vertices. Thus, the diameter of is represented by the Equation 2‑1.

|  |  |  |
| --- | --- | --- |
|  |  | 2‑ |

Here, the diameter is the maximum over all shortest path distances for every pair of vertices and in the graph [56]. In the case of a disconnected graph, where there exist vertices that do not have a path between them, the diameter is often defined as infinity. For a graph containing only a single vertex, the diameter is defined as 0. The concept of the diameter of a graph is applied in numerous applications, such as in network design and analysis, devising algorithms for effective information routing in distributed systems, and in discerning the structure of social networks among others [57]. It's important to note that the process of calculating the diameter of a graph can be computationally expensive, particularly for large graphs. A number of algorithms have been developed to compute the diameter of a graph, which include but are not limited to, the Floyd-Warshall algorithm and Johnson’s algorithm [56].

### Average Distance

The average distance in a graph, also known as the average path length or the characteristic path length, is another crucial concept in graph theory. This metric gives an indication of the overall navigability and connectivity of the graph. Formally, the average distance is the mean shortest path length between all pairs of vertices in the graph. That is, it represents the expected distance between two vertices chosen uniformly at random [57]. The average distance L of G can be given by the formula stated in Equation 2‑2.

|  |  |  |
| --- | --- | --- |
|  |  | 2‑ |

Here, the sum is over all pairs of distinct vertices, and n is the number of vertices in the graph. Essentially, we are summing up the shortest path distances between all pairs of vertices and then dividing by the total number of such pairs [56]. The average distance is a critical metric in understanding the properties of real-world networks, which often exhibit the small-world property. The small-world property describes networks where the average path length is relatively small, meaning that one can get from any given node to any other node in the network through a small number of steps [57]. It's important to note that the average distance only makes sense for connected graphs, where a path exists between every pair of vertices. If a graph is not connected, this metric can't be defined without modification.

### Average Clustering

The average clustering coefficient is an essential measure in the field of graph theory, frequently used to evaluate the tendency of nodes in a network to cluster together. It provides insights into the overall clustering of the graph and the interconnectedness of its nodes. The clustering coefficient of a single node in a graph quantifies how close its neighbors are to being a complete graph. A complete graph is one where every pair of vertices is connected by a unique edge. The average clustering coefficient is simply the mean of the clustering coefficients of all the nodes in the graph [57]. To be more precise, let Kv denote the number of vertices that are neighbors of v, and let Ev denote the number of edges between the neighbors of v. The clustering coefficient Cv for the node v is given by:

Cv = 2Ev / Kv(Kv - 1)

The average clustering coefficient C of the graph is then calculated as:

C = Σ Cv / n

Here, the sum is over all vertices in the graph, and n is the total number of vertices [56]. The average clustering coefficient measures the degree to which nodes in a graph tend to cluster together. It has found widespread application in the study of various types of networks, such as social networks, biological networks, and the World Wide Web, among others [57]. In calculating the average clustering coefficient, it is important to note that it is typically only defined for nodes with at least two neighbors, since the denominator of the formula for Cv would be zero for nodes with fewer than two neighbors. Computing the average clustering coefficient can be a computationally intensive task, especially for larger networks. Various algorithms have been developed to more efficiently calculate it, but the computational complexity is generally high due to the need to examine the local neighborhood of each node [56].

## Genetic Algorithm[[1]](#footnote-2)

Genetic Algorithms (GAs) are a family of search and optimization techniques inspired by the concept of natural selection [58]. Throughout time, GAs have been effectively used to resolve a vast variety of engineering challenges, covering function optimization, machine learning, and scheduling, as cited in reference [59]. This section provides a comprehensive overview of Genetic Algorithms, addressing their theoretical basis, elements, and variants. It also points out the positive and negative aspects of GAs.

The theoretical inspiration of GAs is based on the fundamental principles of biological evolution. According to Darwin's theory of evolution, the most physically fit people are chosen for reproduction, passing on their qualities to the next generation. Over a period of time, this phenomenon results in the acclimatization of species to their surroundings, thereby enhancing their likelihood of survival.

In GAs, a population consists of a set of potential solutions, each referred to as an individual. Genetic operators such as selection, crossover, and mutation are applied to this population. There operators simulate an evolutionary process that occurs over multiple generations [58]. The iterative nature of GAs enables efficient search space exploration and convergence to optimal or near-optimal solutions [60].

### Process

**Representation** is an essential component of Genetic Algorithms, as it defines how potential solutions are encoded for the manipulation within the algorithm. The format that is used the most often is the binary string, where each possible answer is represented as a series of binary digits (0s and 1s) [58]. According to the nature of the issue, different representations, such as real-valued vectors, integers, and permutations, may also be utilized [59].

An **initial population** of potential solutions is created during the startup phase (cf. Figure 1). Both random and domain-specific information may be used to create this population [61]. The choice of population size is based on the complexity of the issue at hand and the preferred ratio of exploitation to exploration [62].

|  |
| --- |
|  |
| Figure 1: Initial population on Wave function |

The **fitness function** is a way to measure the “quality” of each individual in the population. It acts as a gauge of how effectively the solution fulfills both the objectives and the constraints of the challenge [58]. The fitness function must be created to represent the intended result and to direct the search for the best solutions [63].

**Selection** is the process of choosing individuals from the present population to engage in reproduction in order to have the population aggregate around an ideal solution (cf. Figure 2). This mechanism has a preference for those with greater levels of fitness, which is consistent with the concept of "survival of the fittest" [58]. Numerous selection methods have been put forward in the literature, including proportional selection [59], tournament selection [64], and ranking-based selection [65], have been proposed in the literature.

|  |
| --- |
|  |
| Figure 2: Selected individuals from the initial population (cf. Figure 1). The individuals closest to the peak are preserved since they have the best fitness |

The act of integrating the genetic material from two parent solutions to produce one or more child solutions is known as a **crossover**, often referred to as recombination. Crossover aims to explore the search area by developing new solutions that may have higher fitness values [58]. Common crossover operators include single-point, multi-point, and uniform crossover [59].

**Elitism** is an optional element of genetic algorithms that guarantees the preservation of the best person(s), called incumbent, in each generation [60]. Elitism works to stop the loss of the best solutions brought on by genetic operators (e.g., crossover) and to direct search efforts in the direction of the ideal solution by keeping a copy of the fittest individual(s) [59].

### Variants

In order to improve their efficiency and customize them for certain problem domains, many variations of genetic algorithms have been presented. Below is a discussion of a few of the more common variations:

* Real-valued Genetic Algorithms (RVGAs): employ real-valued representations rather than binary strings, enabling a more accurate and effective description of certain problem domains [66]. Arithmetic crossover [67] and non-uniform mutation [68] are two examples of the specific crossover and mutation operators needed for RVGAs.
* Constraint-Handling Techniques: GAs must take into account restrictions in order to effectively solve optimization issues in the real world. Numerous methods for addressing constraints have been put forward, such as penalty functions [69], repair algorithms [70], and multi-objective approaches [63].
* Hybrid Genetic Algorithms (HGAs): combine GAs with additional optimization methods to enhance convergence and search effectiveness [71]. Hill climbing or simulated annealing are two examples of local search techniques that are often used into HGAs to improve the solutions produced by GAs [72].
* Parallel Genetic Algorithms (PGAs): make use of GAs' built-in parallelism to improve performance [73]. PGAs may be implemented using a variety of parallelization techniques, including island models, fine-grained parallelization, and global parallelization.

### Strengths and Weakness of Genetic Algorithms

Strengths:

* Global search capability: due to their lower propensity to get stuck in local optima than gradient-based approaches, GAs are well-suited for identifying global optima in complicated search domains [59].
* Applicability: GAs can be applied to a wide range of optimization problems, as they only require the definition of a fitness function and an appropriate representation [58].
* Robustness: GAs are resilient and simple to apply in real-world problems since they are comparatively insensitive to parameter selection [60].
* Parallelism: GAs may be significantly speed up by leveraging parallel computer resources since they are inherently parallelizable [73].

Weakness:

* Slow convergence: GAs may take a while to converge, particularly in cases where the search spaces are big and complex, or the population is huge [59].
* Premature convergence: GAs can sometimes converge prematurely to suboptimal solutions, particularly if the selection pressure is too high or the mutation rate is too low [60].
* Problem-dependent performance: depending on the problem domain and the selected representation, crossover, and mutation operators, the performance of GAs might vary dramatically [59].

Parameter tuning: although GAs are generally reliable, determining the ideal set of parameters for a given issue may be difficult and time-consuming [62].

## Interpolations Methods

Test

## Model Overview

### Initial Population

The ongoing transition towards sustainable transportation solutions has been marked by the proliferation of electric vehicles (EVs). However, a critical challenge remains in ensuring an adequate and efficiently distributed network of charging stations. This study addresses this challenge by utilizing Machine Learning (ML) techniques, specifically RandomForest (RF) and K-Nearest Neighbors (KNN), to predict the optimal locations for future charging stations. Machine Learning is a branch of artificial intelligence that learns patterns in data and makes predictions or decisions without explicit programming. RandomForest and K-Nearest Neighbors are two widely-used ML algorithms. RandomForest, a bagging-based ensemble learning technique, builds multiple decision trees and aggregates their outputs, resulting in improved accuracy and control of over-fitting [74]. KNN is a type of instance-based learning or lazy learning, where the function is approximated locally, and all computation is deferred until prediction [75]. It uses the feature similarity approach to predict the values of new data points, which further means that the new point will be assigned a value based on how closely it matches the points in the training set. Initially, both models were trained and tested using a dataset containing information about existing charging stations, including location coordinates and the year of installation. The predictive performance of each model was evaluated based on three metrics: Mean Absolute Error (MAE), Mean Squared Error (MSE), and R2 score. The MAE measures the average magnitude of the errors in a set of predictions, without considering their direction. MSE, similar to MAE, punishes larger errors, which tends to be useful in the real world as it punishes large errors. Lastly, the R2 score, also known as the coefficient of determination, quantifies the proportion of the variance in the dependent variable that is predictable from the independent variable(s) [76]. Upon evaluation, the RandomForest model outperformed KNN on all metrics, suggesting that it is better suited for this prediction task. The RF model achieved an R2 score of 0.921 for latitude and 0.867 for longitude, indicating that it was able to explain approximately 92.1% and 86.7% of the variance in the test dataset for latitude and longitude, respectively. Following the evaluation, the chosen RF model was trained on the entire dataset, divided by year. This process allows for the capture of annual trends in the establishment of charging stations, thereby providing a robust model that accounts for temporal variations. The trained models were then deployed in a genetic algorithm to generate an initial population, which suggests promising sites for new charging stations. Genetic algorithms are a type of optimization algorithm that mimics the process of natural selection, using methods such as mutation and crossover to generate new generations of solutions [58]. In this application, each "individual" represents a potential layout of new charging stations. The predictive models were used to estimate the location of new stations in each federal state, based on the state's proportion of total stations. This approach ensures that the stations are distributed in a way that reflects the historical patterns of station placement, while also considering the need for more stations in areas with higher demand. The integration of predictive models into the genetic algorithm allowed for a data-driven approach to generate initial populations, potentially improving the efficiency and effectiveness of the optimization process. In conclusion, the implementation of ML techniques, particularly RandomForest, in conjunction with genetic algorithms, presents a promising methodology for predicting the optimal placement of EV charging stations. This study adds to the growing body of research on ML-based decision support systems in the field of sustainable transportation.

# Results

Test

## Pre-Processing

The raw dataset, procured from the Federal Network Agency, underwent meticulous preprocessing to render it suitable for subsequent analysis. This preprocessing involved several steps aimed at enhancing the quality and readability of the data, thereby facilitating more accurate and effective analysis. One key aspect of the preprocessing was the elimination of duplicate entries from the dataset. It is not uncommon for datasets, particularly those aggregated from multiple sources or entered manually, to contain duplicate entries. Duplicate entries, if not removed, can lead to redundancy in the data and distort the subsequent analysis. Thus, duplicate entries in the dataset were identified and carefully pruned to create a streamlined and precise representation of the unique electric vehicle charging stations distributed across the regions. Following this, the data underwent a process of transformation aimed at standardizing its structure and making it more conducive to analysis. A prime example of this is the transformation of the '*type\_of\_charger*' variable. The original values, '*Schnellladeeinrichtung*' and '*Normalladeeinrichtung*', were remapped to 'fast' and 'normal' respectively. This alteration simplified the task of classifying charging stations based on their charging speed, thereby paving the way for more straightforward subsequent analysis. In the original dataset, geographical coordinates were presented in a format unsuitable for computational processing, with commas employed as decimal points. This posed significant challenges for any computational or spatial analyses that relied on these coordinates. To address this, the commas were replaced with decimal points, and these columns were converted to the float data type. Consequently, calculations involving distances became significantly more straightforward, and the feasibility of creating detailed geospatial visualizations was substantially improved. Another vital transformation step involved the '*commissioning\_date*' column, which stored the commissioning date of each charging station as a string in the day-month-year format. For a more detailed and useful chronological analysis, it was necessary to convert this data into a datetime format. This modification facilitated an overview of the temporal progression of charging station installations, offering valuable insights into their spread over time. Additionally, leading and trailing spaces found in several columns of the dataset were removed to maintain uniformity in the data. Ensuring this consistency was especially important for object columns, such as city names, where minor differences in formatting could lead to inaccurate grouping or comparison of values. The city names present in the dataset were also standardized for improved accuracy and simplicity. Distinct neighborhoods or districts within a city, initially represented separately, were consolidated under the name of the main city. This step significantly reduced geographical complexity during the analysis, fostering a more coherent representation of data. In a further move to streamline the dataset, certain columns containing public keys were dropped. Although these keys are commonly used for cryptographic operations, they were deemed irrelevant to the intended study and were therefore excluded from the dataset, leading to a more simplified data structure. In the final stage of preprocessing, the refined dataset was saved into a new CSV file termed '*ChargingStationCleaned.csv*'. This file stands as a meticulously cleaned and preprocessed version of the original dataset, primed for a detailed examination of the distribution, characteristics, and evolution of electric vehicle charging stations across Germany.

## Data analysis

Test




Figure 3: Cumulative histogram per year




Figure 4: Cumulative histogram per year divided into Normal and Fast charging




Figure 5: Power clustering histogram per year




Figure 6: Charging Type clustering per year

## Network construction

To further scrutinize the distribution and accessibility of electric vehicle charging stations across various geographical regions, a meticulous process for network creation was deployed. The outcome was a detailed and comprehensive graphical representation, visualizing connections between the charging stations for specified years and within user-determined distance parameters. Several programming libraries, each with a unique role, were brought into play in this complex process. The sqlite3 library provided the means for interaction with a SQLite database. The requests library was employed to handle HTTP requests required for distance calculation, whereas the math library was used to compute intricate mathematical operations, including trigonometric functions necessary for distance calculations. The urllib3 library, an HTTP client for Python, managed and streamlined HTTP protocol details. The Transformer module from the pyproj library was crucial for geographic coordinate conversions. An important part of this procedure was the calculation of the Haversine distance, a method utilized to determine the 'great-circle' distance between two points on the Earth's surface given their longitudes and latitudes. Here, the Earth was assumed to be a perfect sphere, and its radius was taken as 6371 kilometers. The function get\_osrm\_distance was developed for more accurate distance measurements. This function initially made a quick estimation based on the Haversine formula. If this approximated distance was found to be less than or equal to 100 kilometers, the Open-Source Routing Machine (OSRM) service was employed. OSRM is an open-source service that uses data from the OpenStreetMap project to find the shortest routes between coordinates. Efficiency and speed were prioritized by creating a SQLite database named 'distances.db', intended to save previously calculated distances. This efficient system considerably reduced the need for repetitive API calls to the OSRM service. If a previously calculated distance value was found in the database, it was retrieved and returned. If not, the function executed an API call to the OSRM service, acquired the precise distance, and subsequently stored this new distance value in the database for future use. The subsequent phase of the process was encapsulated in the create\_network function. This function utilized the previously described distance calculations to construct an undirected graph, which served as a representation of the network of charging stations for a particular year and within a user-specified distance threshold. Each node in the graph corresponded to an electric vehicle charging station, assigned with specific attributes like latitude, longitude, and federal state. Edges between these nodes were added based on the distance between them, calculated by the get\_osrm\_distance function. After the graph's construction, it was visualized on a map. For geographical reference, the boundaries of Germany were used as a backdrop. These boundaries were acquired from a GeoJSON file. The resulting visual output was a graph overlaid on Germany's geographic boundaries, portraying the spread of charging stations and the connectivity between them. The final phase of this process was storing the constructed graph for future uses. The graph was saved in the GraphML format, a comprehensive and easy-to-use file format for graphs, enabling potential future network analysis. Moreover, a visual representation of the graph was saved as a PNG image. This image served as an easily accessible, ready-to-view snapshot of the network for the designated year and distance threshold, aiding in immediate analysis and comparison.

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **Year** | **Diameter** | **Average Distance** | **Average Clustering** | **Density** | **Total nodes** | **Subnetwork size** |
| 2009 | 1.00 | 15.10 | 0.93 | 1.00 | 60 | [2, 2, 23, 4, 26] |
| 2010 | 4.20 | 36.71 | 0.90 | 0.64 | 130 | [14, 77, 38] |
| 2011 | 8.27 | 41.38 | 0.86 | 0.42 | 320 | [256, 61] |
| 2012 | 11.00 | 43.65 | 0.85 | 0.18 | 494 | [494] |
| 2013 | 11.96 | 47.52 | 0.83 | 0.17 | 615 | [613, 2] |
| 2014 | 12.00 | 51.92 | 0.81 | 0.15 | 861 | [861] |
| 2015 | 11.00 | 50.75 | 0.80 | 0.11 | 1393 | [1393] |
| 2016 | 11.00 | 51.70 | 0.78 | 0.10 | 2503 | [2503] |
| 2017 | 10.00 | 53.26 | 0.77 | 0.09 | 4350 | [4350] |
| 2018 |  |  |  |  |  |  |
| 2019 |  |  |  |  |  |  |
| 2020 |  |  |  |  |  |  |
| 2021 |  |  |  |  |  |  |
| 2022 |  |  |  |  |  |  |

Table 1: Characteristics of the different network created

|  |  |
| --- | --- |
|  |  |
| (2009) | (2010) |
|  |  |
| (2011) | (2012) |
|  |  |
| (2013) | (2014) |
|  |  |
| (2015) | (2016) |
|  |  |
| (2017) | (2018) |
|  |  |
| (2019) | (2020) |
|  |  |
| (2021) | (2022) |

Figure 7: Evolution of the charging station network in Germany from 2009 to 2022

## Optimization

Test

# Conclusion and Further Implementations

# Bibliography

|  |  |
| --- | --- |
| [1] | S. Jordan, D. Newport, S. Sandland and P. Vandergert, "Impact of Public Charging Infrastructure on the Adoption of Electric Vehicles," University of East London, 2020. |
| [2] | E. Kontou, C. Liu, F. Xie, X. Wu and Z. Lin, "Understanding the Linkage between Electric Vehicle Charging Network Coverage and Charging Opportunity Using GPS Travel Data," 2019. |
| [3] | B. Haidar and M. T. A. Rojas, "The relationship between public charging infrastructure deployment and other socio-economic factors and electric vehicle adoption in France," *Research in Transportation Economics, DOI: 10.1016/j.retrec.2022.101208.,* vol. 95, 2022. |
| [4] | S. A. Funke, F. Sprei, T. Gnann and P. Plötz, "How much charging infrastructure do electric vehicles need? A review of the evidence and international comparison," *Transportation Research Part D: Transport and Environment,* vol. 77, pp. 224-242, 2019. |
| [5] | T. Franke and J. F. Krems, "Understanding charging behaviour of electric vehicle users," *Transportation Research Part F: Traffic Psychology and Behaviour,* vol. 21, pp. 75-89, 2013. |
| [6] | N. S. Pearre, W. Kempton, R. L. Guensler and V. V. Elango, "Electric vehicles: How much range is required for a day’s driving?," *Transportation Research Part C: Emerging Technologies,* vol. 19, no. 6, pp. 1171-1184, 2011. |
| [7] | W. Sierzchula, S. Bakker, K. Maat and B. van Wee, "The influence of financial incentives and other socio-economic factors on electric vehicle adoption," *Energy Policy,* vol. 68, pp. 183-194, 2014. |
| [8] | O. Egbue and S. Long, "Barriers to widespread adoption of electric vehicles: An analysis of consumer attitudes and perceptions," *Energy Policy,* vol. 48, pp. 717-729, 2012. |
| [9] | Y. Zhang, Y. Yu and B. Zou, "Analyzing public awareness and acceptance of alternative fuel vehicles in China: The case of EV," *Energy Policy,* vol. 39, no. 11, pp. 7015-7024, 2011. |
| [10] | W. Kong, Y. Luo, G. Feng, K. Li and H. Peng, "Optimal location planning method of fast charging station for electric vehicles considering operators, drivers, vehicles, traffic flow and power grid," *Energy,* vol. 186, 2019. |
| [11] | M. C. Falvo, R. Lamedica, R. Bartoni and G. Maranzano, "Energy management in metro-transit systems: An innovative proposal toward an integrated and sustainable urban mobility system including plug-in electric vehicles," *Electric Power Systems Research,* vol. 81, no. 12, pp. 2127-2138, 2011. |
| [12] | S. Guo and H. Zhao, "Optimal site selection of electric vehicle charging station by using fuzzy TOPSIS based on sustainability perspective," *Applied Energy,* vol. 158, pp. 390-402, 2015. |
| [13] | J. Asamer, M. Reinthaler, M. Ruthmair, M. Straub and J. Puchinger, "Optimizing charging station locations for urban taxi providers," *Transportation Research Part A: Policy and Practice,* vol. 85, pp. 233-246, 2016. |
| [14] | Z. Zhu, Z. Gao, J. Zheng and H. Du, "Charging Station Planning for Plug-In Electric Vehicles," *Journal of Systems Science and Systems Engineering,* vol. 27, pp. 24-45, 2018. |
| [15] | Z. Sun, W. Gao, B. Li and L. Wang, "Locating charging stations for electric vehicles," *Transport Policy,* vol. 98, pp. 48-54, 2020. |
| [16] | I. Frade, A. Ribeiro and A. Antunes, "Optimal Location of Charging Stations for Electric Vehicles in a Neighborhood in Lisbon, Portugal," *Transportation Research Record: Journal of the Transportation Research Board,* vol. 2252, no. 1, 2011. |
| [17] | F. He, Y. Yin and J. Zhou, "Deploying public charging stations for electric vehicles on urban road networks," *Transportation Research Part C: Emerging Technologies,* vol. 60, pp. 227-240, 2015. |
| [18] | N. Shahraki, H. Cai, M. Turkay and M. Xu, "Optimal locations of electric public charging stations using real world vehicle travel patterns," *Transportation Research Part D: Transport and Environment,* vol. 41, pp. 165-176, 2015. |
| [19] | F. Wu and R. Sioshansi, "A stochastic flow-capturing model to optimize the location of fast-charging stations with uncertain electric vehicle flows," *Transportation Research Part D: Transport and Environment,* vol. 53, pp. 354-376, 2017. |
| [20] | W. Tu, Q. Li, Z. Fang, S. Shaw, B. Zhou and X. Chang, "Optimizing the locations of electric taxi charging stations: A spatial–temporal demand coverage approach," *Transportation Research Part C: Emerging Technologies,* vol. 65, pp. 172-189, 2016. |
| [21] | L. Luo, W. Gu, S. Zhou, H. Huang, S. Gao, J. Han, Z. Wu and X. Dou, "Optimal planning of electric vehicle charging stations comprising multi-types of charging facilities," *Applied Energy,* vol. 226, pp. 1087-1099, 2018. |
| [22] | K. Liu, L. Kang, H. Ma, J. Zhang and Q. Peng, "Multi-objective optimization of charging patterns for lithium-ion battery management," *Energy Conversion and Management,* vol. 159, pp. 151-162, 2018. |
| [23] | H. Mehrjerdi and R. Hemmati, "Electric vehicle charging station with multilevel charging infrastructure and hybrid solar-battery-diesel generation incorporating comfort of drivers," *Journal of Energy Storage,* vol. 26, 2019. |
| [24] | Y. He, Z. Song and Z. Liu, "Fast-charging station deployment for battery electric bus systems considering electricity demand charges," *Sustainable Cities and Society,* vol. 48, 2019. |
| [25] | S. Davidov and M. Pantos, "Optimization model for charging infrastructure planning with electric power system reliability check," *Energy,* vol. 166, pp. 886-894, 2019. |
| [26] | S. Hosseini and M. Sarder, "Development of a Bayesian network model for optimal site selection of electric vehicle charging station," *International Journal of Electrical Power & Energy Systems,* vol. 105, pp. 110-122, 2019. |
| [27] | R. Chen, X. Qian, L. Miao and S. V. Ukkusuri, "Optimal charging facility location and capacity for electric vehicles considering route choice and charging time equilibrium," *Computer & Operations Research,* vol. 113, 2020. |
| [28] | T. Zeng, S. Bae, B. Travacca and S. Moura, "Inducing Human Behavior to Maximize Operation Performance at PEV Charging Station," *IEEE Transactions on Smart Grid,* vol. 12, no. 4, pp. 3353-3363, 2021. |
| [29] | M. J. Hodgson, "A Flow Capturing Location Allocation Model," *Geographical Analysis,* vol. 22, no. 3, pp. 270-279, 1990. |
| [30] | M. Kuby and S. Lim, "The flow-refueling location problem for alternative-fuel vehicles," *Socio-Economic Planning Sciences,* vol. 39, no. 2, pp. 125-145, 2005. |
| [31] | C. Upchurch and M. Kuby, "A Model for Location of Capacitated Alternative-Fuel Stations," *Geographical Analysis,* vol. 41, no. 1, pp. 85-106, 2009. |
| [32] | M. Hosseini and S. A. MirHassan, "A heuristic algorithm for optimal location of flow-refueling capacitated stations," *International Transactions in Operational Research,* vol. 24, pp. 1377-1403, 2017. |
| [33] | B. Yildiz, B. Arslan and O. E. Karaan, "A branch and price approach for routing and refueling station location model," *European Journal of Operational Research,* vol. 248, no. 3, pp. 815-826, 2016. |
| [34] | S. Li, Y. Huang and S. J. Mason, "A multi-period optimization model for the deployment of public electric vehicle charging stations on network," *Transportation Research Part C,* vol. 65, pp. 128-143, 2016. |
| [35] | Y. W. Wang and C. C. Lin, "Locating multiple types of recharging stations for battery-powered electric vehicle transport," *Transportation Research Part E,* vol. 58, pp. 76-87, 2013. |
| [36] | O. Arslan and O. E. Karasan, "A Benders decomposition approach for the charging station location problem with plug-in hybrid electric vehicles," *Transportation Research Part B,* vol. 93, pp. 670-695, 2016. |
| [37] | M. Ghamami, A. Zockaie and Y. M. Nie, "general corridor model for designing plug-in electric vehicle charging infrastructure," *Transportation Research Part C,* vol. 68, pp. 389-402, 2016. |
| [38] | S. H. Chung and C. Kwon, "Multi-period planning for electric car charging station locations: a case of Korean expressways," *European Journal of Operational Research,* vol. 242, no. 2, pp. 677-687, 2015. |
| [39] | A. Zhang, J. Kang and C. Kwon, "Incorporating demand dynamics in multi-period capacitated fast-charging location planning for electric vehicles," *Transportation Research Part B,* vol. 103, pp. 5-29, 2017. |
| [40] | H. De Vries and H. Duijzer, "Incorporating driving range variability in network design for refueling facilities," *Omega,* vol. 69, pp. 102-114, 2017. |
| [41] | C. Lee and J. Han, "Benders-and-price approach for electric vehicle charging station location problem under probabilistic travel range," *Transportation Research Part B,* vol. 106, pp. 130-152, 2017. |
| [42] | M. Hosseini and S. A. MirHassani, "Refueling-station location problem under uncertainty," *Transportation Research Part E,* vol. 84, pp. 101-116, 2015. |
| [43] | F. Wu and R. Sioshansi, "A stochastic flow-capturing model to optimize the location of fast-charging stations with uncertain," *Transportation Research Part D,* vol. 53, pp. 354-376, 2017. |
| [44] | M. Miralinaghi, Y. Lou, B. B. Keskin and A. Zarrinmehr, "Refueling station location problem with traffic deviation considering route choice and demand uncertainty," *International Journal of Hydrogen Energy,* vol. 42, no. 5, pp. 3335-3351, 2017. |
| [45] | P. Sadeghi-Barzani, A. Rajabi-Ghahnavieh and H. Kazemi-Karegar, "Optimal fast charging station placing and sizing," *Applied Energy,* vol. 125, pp. 289-299, 2014. |
| [46] | O. Arslan and O. Karasan, "A Benders decomposition approach for the charging station location problem with plug-in hybrid electric vehicles," *Transportation Research Part B: Methodological,* vol. 93, no. A, pp. 670-695, 2016. |
| [47] | K. Zhang, L. Xu, M. Ouyang, H. Wang, L. Lu, J. Li and Z. Li, "Optimal decentralized valley-filling charging strategy for electric vehicles," *Energy Conversion and Management,* vol. 78, pp. 537-550, 2014. |
| [48] | Z. Zhu, Z. Gao, J. Zheng and H. Du, "Charging station location problem of plug-in electric vehicles," *Journal of Transport Geography,* vol. 52, pp. 11-22, 2016. |
| [49] | M. Akbari, M. Brenna and M. Longo, "Optimal Locating of Electric Vehicle Charging Stations by Application of Genetic Algorithm," *Sustainability,* vol. 10, no. 4, 2018. |
| [50] | A. Awasthi, K. Venkitusamy, S. Padmanaban, R. Selvamuthukumaran, F. Blaabjerg and A. K. Singh, "Optimal planning of electric vehicle charging station at the distribution system using hybrid optimization algorithm," *Energy,* vol. 113, pp. 70-78, 2017. |
| [51] | Y. Chen, C. Cheng, S. Li and C. Yu, "Location optimization for multiple types of charging stations for electric scooters," *Applied Soft Computing,* vol. 67, pp. 519-528, Applied Soft Computing. |
| [52] | Y. Zhang, Q. Zhang, A. Farnoosh, S. Chen and Y. Li, "GIS-Based Multi-Objective Particle Swarm Optimization of charging stations for electric vehicles," *Energy,* vol. 169, pp. 844-853, 2019. |
| [53] | M. Straka and L. Buzna, "Clustering algorithms applied to usage related segments of electric vehicle charging stations," *Transportation Research Procedia,* vol. 40, pp. 1576-1582, 2019. |
| [54] | Y. Wu, A. Ravey, D. Chrenko and A. Miraoui, "Demand side energy management of EV charging stations by approximate dynamic programming," *Energy Conversion and Management,* vol. 196, pp. 878-890, 2019. |
| [55] | R. Diestel, Graph Theory, Springer, 2010. |
| [56] | T. H. Cormen, C. E. Leiserson, R. L. Rivest and C. Stein, Introduction to algorithms, MIT Press, 2009. |
| [57] | M. Newman, Networks: An Introduction, Oxford University Press, 2010. |
| [58] | H. Holland, Adaptation in Natural and Artificial Systems: An Introductory Analysis with Applications to Biology, Control, and Artificial Intelligence, MIT Press Direct, 1992. |
| [59] | D. E. Goldberg, Genetic Algorithms in Search, Optimization and Machine Learning, Addison-Wesley Longman Publishing Co., Inc., 1989. |
| [60] | K. De Jong, "An Analysis of the Behavior of a Class of Genetic Adaptive Systems," Department of Computer and Communication Sciences, University of Michigan, 1975. |
| [61] | M. Mitchell, An Introduction to Genetic Algorithms, MIT Press, 1998. |
| [62] | A. E. Eiben and J. E. Smith, Introduction to Evolutionary Computing, Springer, 2003. |
| [63] | K. Deb, Multiobjective Optimization Using Evolutionary Algorithms, Jhon Wiley and Sons Ltd, 2001. |
| [64] | B. L. Miller and D. E. Goldberg, "Genetic Algorithms, Tournament Selection and the Effects of Noise," *Complex Symstems,* vol. 9, pp. 193-212, 1995. |
| [65] | J. E. Baker, "Adaptive Selection Methods for Genetic Algorithms," in *Proceedings of the 1st International Conference on Genetic Algorithms*, 1985. |
| [66] | A. H. Wright, "Genetic Algorithms for Real Parameter Optimization," *Foundations of Genetic Algorithms,* vol. 1, pp. 205-2018, 1991. |
| [67] | K. Deb and R. B. Agrawal, "Simulated Binary Crossover for Continuous Search Space," *Complex Systems,* vol. 9, no. 2, pp. 115-148, 1995. |
| [68] | Z. Michalewicz, Genetic Algorithms + Data Structures = Evolution Programs, Springer, 1996. |
| [69] | A. E. Smith and D. W. Coit, Constraint-Handling Techniques - Penalty Functions, Handbook of Evolutionary Computation, Institute of Physics Publishing and Oxford, 1997. |
| [70] | J. C. Bean, "Genetic Algorithms and Random Keys for Sequencing and Optimization," *ORSA Journal on Computing,* vol. 6, no. 2, 1994. |
| [71] | X. Yao, Y. Liu and G. Lin, "Evolutionary programming made faster," *IEEE Transactions on Evolutionary Computation, DOI: 10.1109/4235.771163,* vol. 3, no. 2, pp. 82-102, 1999. |
| [72] | D. E. Goldberg and S. Voessner, "Optimizing global-local search hybrids," in *GSECCO'99*, 1999. |
| [73] | E. Cantú-Paz, Efficient and Accurate Parallel Genetic Algorithms, Springer, 2001. |
| [74] | L. Breiman, "Random Forests," *Machine Learning,* vol. 45, pp. 5-32, 2001. |
| [75] | D. W. Aha, D. Kibler and M. K. Albert, "Instance-based learning algorithms," *Machine Learning,* vol. 6, pp. 37-66, 1991. |
| [76] | R. J. Hyndman and A. B. Koehler, "Another look at measures of forecast accuracy," *International Journal of Forecasting,* vol. 22, no. 4, pp. 679-688, 2006. |
| [77] | G. Filomeno, "Automation of Design Synthesis for Electric Vehicle Transmissions," Ruhr-Universität Bochum, Ph.D. Thesis, Bochum, 2023. |

**Insurance**

I certify that I have written the above thesis independently and have not used any outside help. All passages taken verbatim or in spirit from published or unpublished literature have been marked as such.

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Name

**Blocking notice**

Inspection of the thesis " *Analysis and Optimization of the Charging Station Network in Germany*" is not permitted. Exceptions to this are the supervising lecturers and the authorised members of the examination board.

Publication and reproduction of the work - even in excerpts - is not permitted up to and including xy.

1. This section is a slightly modified version of the Section 4.2. “Genetic algorithm” of the thesis “Automation of Design Synthesis for Electric Vehicle Transmission” published by the same author of this thesis and has been reproduced here with the permission of the copyright holder [30] [↑](#footnote-ref-2)